| # Speaker Project # Prototyping the Crossover

> > > Now to build the first pass of the crossover we need to create three more network resources, called Woofer, Tweeter, and Both. Having the networks separate like this makes alterations much simpler. Make sure each network has impedance turned on. Also, for the Both network turn on Automatic Overview Chart.

> > > To populate the Woofer network select everything in the Woof network (draw a box around them) then select Edit / Copy (or press Ctrl+C) and copy all of the network components to the clipboard. Go to the Woofer network and select Edit / Paste (or press Ctrl+V) to bring them in. Delete the extra Source component (highlight it and select Edit / Delete or hit the Del key.

> > > Do the same for the Tweeter network. This technique (cutting and pasting between networks will be used a lot as the prototype evolves.

> > > On to the next page.

> > > last updated March 08, 2001